# Milk COLLECTION – Neither Tanker nor Driver Crosses LOS

## For Direct Loads of Milk

### Example SOP – Modify to fit your operation

1. Licensed milk weigher/sampler(s) are employed by the farm eliminating the necessity for the driver to enter the milk house.
2. The on-farm licensed milk weigher/sampler collects milk samples, labels them, places them in a sealed plastic bag, and sprays the exterior of the bag with desired disinfectant.
   1. The bagged samples are placed across the Biosecurity Entry in storage cooler on the exterior side of the LOS where the milk hauler/driver can access them without crossing the LOS.
3. The milk hauler/driver delivers the empty tanker to the open bay and disconnects tractor from empty tanker according to normal protocols
   1. Farm personnel should perform farm-dedicated hose disconnection and sealing activities from inside the milk house, allowing the hauler to stay outside of the LOS.
4. The milk hauler/driver moves tractor to filled tanker and connects the tractor to the tanker following normal protocols.
   1. Farm personnel should ensure that the exterior of the storage compartment and valve area is cleaned and disinfected prior to connection to the farm-dedicated hose.
   2. Farm personnel should perform farm-dedicated hose connection activities from inside the milk house, allowing the hauler to stay outside of the LOS.